RED1-229 - Modification

**TABLE R402.5.1.1 AIR BARRIER, AIR SEALING AND INSULATION INSTALLATIONa**

Portions of table not shown remain unchanged.

|  |  |  |
| --- | --- | --- |
| COMPONENT | AIR BARRIER CRITERIA |  INSULATION INSTALLATION CRITERIA |
|  | ~~Air sealing materials recognized in a listed fire-resistance rated~~ ~~common wall or double wall design and installed in accordance~~ ~~with the listing, or air sealing materials recognized in an~~ ~~approved design, shall be used.~~ |  |
|  | ~~Common walls or double walls shall be considered an exterior~~ ~~wall for the purposes of air barrier and air sealing application of~~ ~~this Table.~~ |  |
| Common walls or double walls separating attached single-family dwellings or townhouses | An interior air barrier shall be provided. Air sealing at the intersections with building thermal envelope shall be provided.Where installed in a fire-resistance rated wall assembly, air sealing materials shall comply with one of the following: | Insulation materials recognized in the *approved* ~~listed~~ common wall or double-wall design and installed in accordance with the ~~listing, or insulation materials recognized in the approved~~ *approved* design~~,~~ shall be permitted to be used. |
|  | 1. be in accordance with an *approved* design for the fire-resistance rated assembly.
2. be supported by *approved* data that shows the assembly as installed complies with the required fire-resistance rating.
 |  |
|  |  |  |